**Selection-Screen Begin Of Block**

En fazla 20 karakter olabilir. SE38 > program oluşturuyoruz.

Tables: sflight.

SELECTION-SCREEN BEGIN OF BLOCK block1 WITH FRAME TITLE 1 NO INTERVALS.

Select-OPTIONS: s\_carrid for sflight-carrid no INTERVALS,

s\_connid for sflight-connid,

s\_fldate for sflight-fldate.

SELECTION-SCREEN END OF BLOCK block1.

INITIALIZATION.

T1= ‘Tirial Title’.

**Selection-Screen Begin Of Screen**

TABLES: sflight.

SELECTION-SCREEN BEGIN OF SCREEN 100 TITLE text-001 as WINDOW.

Selectıon-screen begın of block block1 wıth frame title t1.

Select-options: s\_carrid for sflight-carrid,

S\_connid for sflight-connid,

S\_fldate for sflight-fladate.

SELECTION-SCREEN END OF BLOCK block1.

SELECTION-SCREEN END OF SCREEN 100.

INITIALIZATION.

T1= ‘Block Title’

Call selection-screen 100 startıng at 5 5 ending at 110 50.

**Selection-Screen Subscreen**

TABLES: sscrfields,

Sflight.

\*Subscreen 1

Selection-screen begın of screen 001 as subscreen.

Parameters: p\_carrid type sflight-carrid,

P\_connid type sflight-connid.

Selection-screen end of screen 001.

Selection-screen begın of screen 002 as subscreen.

Parameters: p\_var(10) type c,

P\_var(10) type c.

Selection-screen end of screen 001.

**PARAMETERS:**

P\_carrid type sflight-carrid.

P\_connid type sflight-connid default ‘0017’.

P\_fldate type sflight-fldate OBLIGATORY. //Zorunlu alan işaretidir.

P\_carname type scarr\_carrname LOWER CASE.

P\_carri2 type sflight-carrid no-display.

P\_Carri3 type sflight-carrid vısıble length 10.

PARAMTERES p\_m1 type vs USER-COMMAND x.

AT selectıon-screen OUTPUT.

Loop at screen.

IF screen-name = ‘P\_CARRID’.

IF p\_m1 = abap\_true.

Screen-input = 0.

Endıf.

MODIFY SCREEN.

Endloop.

**CHECKBOX**

Parameters: p\_chkbx as checkbox.

START-OF-SELECTION.

IF p\_chkbx = ‘x’.

Wrıte:/’Checkbox is selected’.

Else.

Write: / ‘Checkbox is not selected’.

ENDIF.

**RADİOBUTTON**

PARAMETERS p\_r\_btn1 radiobutton group rb1.

Parameters p\_r\_btn2 radiobutton group rb1.

START-OF-SELEECTION.

IF p\_r\_btn1 = ‘X’.

Write:/ ‘Radio Button 1 is selected’.

Elseif P\_R\_BTN2 = ‘X’.

Write:/’Radio Button 2 is selected’.

Endif.

**LİSTBOX**

PARAMETERS p\_lstbox TYPE i AS LISTBOX VİSİBLE LENGTH 25.

AT SELECTION-SCREEN OUTPUT.

CALL FUNCTION ‘VRM\_SET\_VALUES’

Exporting

İd= CONV vrm\_id (’P\_LSTBOX’)

Values = VALUE vrm\_values(

FOR İ = 1 UNTİL İ > 10

(key = i text = |VALUE{İ}| )

).

**SELECT OPTIONS**

TABLES: sflight.

SELECT-options: s\_carrid for sflight-carrid.

SELECT-options: s\_carri2 for sflight-carrid DEFAULT ‘AA’.

Select-options: s\_carrid3 for sflight-carrid NO INTERVALS.

**SELECTION TEXT**

Selectıon-screen begın of block b1 with frame title text-001.

PARAMETERS: p\_CARRİD TYPE SFLİGHT-CARRİD.

Selection-screen end of block b1.